/\*

The MIT License (MIT)

Copyright (c) 2022 Robert E Bridges

Permission is hereby granted, free of charge, to any person obtaining a copy of this software and associated documentation files (the "Software"), to deal in the Software without restriction, including without limitation the rights to use, copy, modify, merge, publish, distribute, sublicense, and/or sell copies of the Software, and to permit persons to whom the Software is furnished to do so, subject to the following conditions:

The above copyright notice and this permission notice shall be included in all copies or substantial portions of the Software.

THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.

On a personal note, if you develop an application or product using this library and make millions of dollars, I'm happy for you!

Code by Robert E Bridges

This library is intended to be used to create your own Nextion Library. Most of it is done for you.

The function that you will mostly alter is the "respondToReply()" function.

I developed this library to control the valves in my Home Heating system, so there are functions that pertain to the opening/closing of valves. This can be used as an example as to how to use/develop the Library.

I mostly communicate with the nextion through the passing of data into/from numeric variables.

I have a TimerEvent which runs at 600mS intervals, slow I know but fast enough for my current needs.

When, for example this timer notices that the numeric variable "SetTime" is not zero it takes the value from this variable and sets the time. The format of the data in this variable is (in HEX) "HHMMSS".

After having set the time the variable is set back to 0 again.

Other variables are interrogated and responded to in a similar way by the code for this Timer Event.

An example is to give an impressionof a flashing led, turning on or off a radio button with a different colour for on and off.

Below is the Nextion code snippet to set the RTC time.

//=================================

//Set RTC time if SetTime > 0 NOTE: Variables declared in Nextion Programs.s

//=================================

if(SetTime!=0)

{

xx=SetTime

xx=xx>>16

rtc3=xx // Set the hour

xx=SetTime

xx=xx&0xFF00

xx=xx>>8 // Set the minutes

rtc4=xx

xx=SetTime&0xFF

rtc5=xx // Set the seconds

SetTime=0

}

Revision Date Author Description

1.0 16/04/2022 Robert E Bridges - Initial release

1.1 17/04/2022 Robert E Bridges - Added printMoreTextToNextion and improved explanation.

1.15 18/04/2022 Robert E Bridges - Changed to reflect Nextion use of Global Variables in Program.s

1.20 22/04/2022 Robert E Bridges - Added nextionError. Set when Nextion returns an error or an invalid number of characters

returned

- Added errorCode. Set to the Nextion returned error or thr error code for invalid num chars.

errorCode is cleared if getReply() is called and there are chars from Nextion.

- All the following added:

preserveTopTextLine

writeToTopTextLine

releaseTopTextLine

clearTextScreen

clearTopTextLine

setBackLight

getNumVarValue

setNumVarValue

1.25 01/05/2022 Robert E Bridges - Completed respondToReply. Now handles the return of Text from the Nextion.

- Added setTextBuffer. Adds a text buffer where text data is placed from Nextion.

1.30 08/05/2022 Robert E Bridges - Added askSerialBufferClear use THIS

and isSerialBufferClear before THIS

1.35 09/05/2022 Robert E Bridges - Added setBkcmdLevel and handling of successful command completion when bkcmd = 1 or 3.

see setBkcmdLevel for explanation.

1.40 10/05/2022 Robert E Bridges - Added lastComdCompletedOk as a complement to setBkcmdLevel above.

- Added timeout to getReply

1.50 25/05/2022 Robert E Bridges - Added turnscreenTime

- Changed getNumVarValue error return to -1 from 0xFFFF.

- Added a const char revision to reflect the revision.

duplicated with revisionNum to better allow checking/comparison.

1.55 29/05/2022 Robert E Bridges - Added gotoPage.

1.56 03/06/2022 Robert E Bridges - Inseted MISSING break in Nextion reset code.

1.60 04/06/2022 Robert E Bridges - Added getNumVarFloat and second form of getNumVarValue.

- Added setStrVarValue.

- Added viewDebugText (or NOT).

- Corrected getNumVarValue - previously did not wait long enough for some numbers

- getNumVarValue sets it's own error code on error and also sets nextionError

- Introduced a variable timeout for getNumVarValue, initially at 1000 ms;

- Introduced a variable timeout for getStringVarValue, initially at 1000 ms;

- getNumVarValue sets it's own error code on error and also sets nextionError

- getStringVarValue corrected.

- gotoPage corrected.

- Tidied up various timeout values.

1.65 05/06/2022 Robert E Bridges - Added setNumVarFloat.

1.66 11/04/2023 Robert E Bridges - Minor change to remove compiler warning for Nextion.behin cpp file.\*/

1.67 13/09/2023 Robert E Bridges - Minor change onOffFlashingTyp off, on, flashing changed to ledOn, ledOff, ledFlashing.

- programmer may have used off and on elsewhere and may conflict.

1.68 29/09/2023 Robert E Bridges - setTextBuffer changed from

void setTextBuffer( const char\* textBuffer, uint8\_t textBufferSize);

to

void setTextBuffer( char\* textBuffer, uint8\_t textBufferSize);

1.69 06/02/2024 Robert E Bridges - Added SetDate to complement SetTime.

1.70 18/02/2024 Robert E Bridges - Added variables and functions associated with getting date/time from Nextion:

- added getDateTime() to get date/time from Nextion - works with the NEW example HMI.

- added setMcuDateTimeCallback, - works with the NEW example HMI.

- added variables nextionDateTimeUpdt, packedDateTime - works with the NEW example HMI.

- Added variable and function to get EEprom data from Nextion:

- added fns setEEPromDataBuffer and getEEPromData - works with the NEW example HMI.

- added eepromDataChanged - works with the NEW example HMI.

(\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*)

(\* Below at vs 1.71 is a MAJOR Potential Error Fix \*)

(\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*)

1.71 19/02/2024 Robert E Bridges - GetReply() changed. An error could occur if the Nextion data was coming too fast.

- Added getPage() - works with the NEW example HMI.

1.72 22/02/2024 Robert E Bridges - Added getDaylightSavingOn(), setSystemResetCallback()

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* These are all the data types used to communicate with the Nextion. More correctly \*

\* they are the data types for data returned FROM the Nextion display. \*

\* Some data returns only need 4 bytes, the Id and the Nextion terminating string, \*

\* \0xFF\0xFF\0xFF, whilst others require much more right up to the reset function \*

\* which returns two data sets in one go i.e. startUp message and ready message \*

\* |----- Start up message ----| |- Ready Message -| \*

\* 0x00 0x00 0x00 0xFF 0xFF 0xFF 0x88 0xFF 0xFF 0xFF \*

\* \*

\* All the comms are put int the variable nextionEvent which is of nextionEventType. \*

\* this consists of the Id of the message which is returned in nextionEvent.Id. The \*

\* remaining bytes are put into nextionEvent.reply3, or nextionEvent.reply4 etc. \*

\* The relevant reply type is examined to interpret the data. \*

\* Infact when data is returned from the Nextion it is placed in \*

\* nextionEvent.resetReply because this is the lartgest structure and can accommodate \*

\* all types of reply. \*

\* Note that there is sometimes the need to convert from little endian to big endian \*

\* due to Teensy and Nextion using different endians. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

struct rep3Type {

uint32\_t nextTerm; // = 0xFFFFFF swap little endian to big endian = 0xFFFFFF00

};

struct rep4Type {

uint8\_t pageNum;

uint32\_t nextTerm;

};

struct rep5Type {

uint8\_t ans[2];

uint32\_t nextTerm;

};

struct rep6Type {

uint8\_t pageNum;

uint8\_t component;

uint8\_t pressed;

uint32\_t nextTerm;

};

struct rep7Type {

union {

uint8\_t ans[4];

uint16\_t num[2];

uint32\_t number32bit;

};

uint32\_t nextTerm;

};

struct rep7IntType {

union {

uint8\_t ans[4];

uint16\_t num[2];

int32\_t number32bitInt;

};

uint32\_t nextTerm;

};

struct rep8Type {

union {

uint8\_t x[2];

uint16\_t xPos;

};

union {

uint8\_t y[2];

uint16\_t yPos;

};

uint8\_t pressed;

uint32\_t nextTerm;

};

// After Reset Nextion Returns 00 00 00 FF FF followed by 88 FF FF FF

struct resetReplyType { // first 00 in nextionEvent char Id

uint32\_t startup4Bytes; // 00 00 FF FF swap little endian to big endian = 0x0FFFF0000

uint8\_t startupByte; // FF

uint32\_t readyReply; // 88 FF FF FF swap little endian to big endian = 0x0FFFFFF88

uint32\_t overflow; // Just to allow a 4 byte buffer if extra erroneous bytes are

}; // sent during "reset" (Have Seen It in error conditions)

struct nextionEventType {

char id;

union {

rep3Type reply3;

rep4Type reply4;

rep5Type reply5;

rep6Type reply6;

rep7Type reply7;

rep7IntType reply7int;

rep8Type reply8;

resetReplyType resetReply; //-- The largest Type

uint8\_t data[sizeof(resetReplyType)]; // Just so that data can be analysed for debug purposes

};

}; // nextionEvent;

#pragma pack(pop)

enum onOffFlashingType {

off = 0,

on, // = 1,

flashing // = 2

};

enum topMidBottmType {

top = 0,

mid, // = 1,

bottom // = 2,

};

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* \*

\* This is an explanation of the data returned from the Nextion. \*

\* I think it's self explanatory, but then I wrote it!! \*

\* There is the Id returned by the Nextion, followed by the number of following bytes,\*

\* followed by an explanation of those bytes. It is only because we have this \*

\* information that this library was able to be written. All is based upon this info. \*

\* \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\* /-------- Id Codes Returned by Nextion

/

/ /----------- Number of Char/Bytes returned after Id Char/Byte

/ /

/ / /-------- Char/Bytes returned after Id Char/Byte / / /

/ / |-------------------------------------| \*/

const uint8\_t nextionStartUp = 0x00; // 5 0x00 0x00 0x00 0xFF 0xFF 0xFF Returned when Nextion has started or

// reset

const uint8\_t instructionSuccess = 0x01; // 3 0x01 0xFF 0xFF 0xFF (ONLY SENT WHEN bkcmd = 1 or 3)

const uint8\_t touchEvent = 0x65; // 6 0x65 0x00 0x01 0x01 0xFF 0xFF 0xFF Returned when Touch occurs

// data: Page 0, Component 1, Pressed Returns page, component and pressed

// or not, 0 or 1

const uint8\_t currentPageNumber = 0x66; // 4 0x66 0x01 0xFF 0xFF 0xFF Returned when the sendme command is used.

// data : page 1

const uint8\_t touchCoordinateAwake = 0X67; // 8 0x67 0x00 0x7A 0x00 0x1E 0x01 0xFF 0xFF 0xFF Returned when sendxy = 1 and not

// data: (122, 30) Pressed in sleep mode

const uint8\_t touchCoordinateSleep = 0X68; // 8 0x68 0x00 0x7A 0x00 0x1E 0x01 0xFF 0xFF 0xFF Returned when sendxy = 1 and

// data: (122, 30) Pressed (0 for NOT pressed) exiting sleep

//

const uint8\_t stringDataEnclosed = 0x70; // 0 means variable amount

// 0x70 0x61 0x62 0x31 0x32 0x33 0xFF 0xFF 0xFF Returned when using get command

// data: ab123 for string.

// Each byte is converted to char.

const uint8\_t numericDataEnclosed = 0x71; // 7 0x71 0x01 0x02 0x03 0x04 0xFF 0xFF 0xFF Returned when get command to

// data: 67305985 return a number

// 4 byte 32 bit value in little endian Order.

const uint8\_t autoEnteredSleepMode = 0x86; // 3 0x86 0xFF 0xFF 0xFF Returned when Nextion enters sleep

// automatically.

// Using sleep = 1 will not return an 0x86

const uint8\_t autoAwakeFromSleepMode = 0x87; // 3 0x87 0xFF 0xFF 0xFF Returned when Nextion leaves sleep

// automatically

// Using sleep = 0 will not return an 0x87

const uint8\_t nextionReady = 0x88; // 3 0x88 0xFF 0xFF 0xFF Returned when Nextion has powered up and is

// now initialized successfully

const uint8\_t powerOnMicroSDCardDet = 0x89; // 3 0x89 0xFF 0xFF 0xFF Returned when power on detects inserted

// microSD and begins Upgrade by microSD process.

const uint8\_t transparentDataFin = 0xFD; // 3 0xFD 0xFF 0xFF 0xFF Returned when all requested bytes of

// Transparent Data mode have been received,

// and is now leaving transparent data mode

// (See 1.16)

const uint8\_t transparentDataReady = 0xFE; // 3 0xFE 0xFF 0xFF 0xFF Returned when requesting Transparent Data

` // mode, and device is now ready to begin

// (see 1.16) receiving the specified quantity of data

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* \*

\* Below are the error codes returned by the Nextion \*

\* Whether they are returned or not depends upon the value by the Nextion bkcmd. \*

\* This can be set to Level 0 ... to Level 3. Below are shown the bkcmd level at which \*

\* the error/state message is returned. The default is Level 2. \*

\* \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\* Error/event codes (ONLY 0x01 is an event code)

/------------ Error/Event Code

/

/ /------- Error/Event Code returned when bkcmd equals value shown

/ /

/ |--------| \*/

const uint8\_t invalidInstruction = 0x00; // bkcmd 2,3 0x00 0xFF 0xFF 0xFF Returned when instruction sent by user has failed

//const uint8\_t instructionSuccess = 0x01; // bkcmd 1,3 0x01 0xFF 0xFF 0xFF (ONLY SENT WHEN bkcmd = 1 or 3 )

const uint8\_t invalidComponentId = 0x02; // bkcmd 2,3 0x02 0xFF 0xFF 0xFF Returned when invalid Component ID or name was used

const uint8\_t invalidPageId = 0x03; // bkcmd 2,3 0x03 0xFF 0xFF 0xFF Returned when invalid Page ID or name was used

const uint8\_t invalidPictureId = 0x04; // bkcmd 2,3 0x04 0xFF 0xFF 0xFF Returned when invalid Picture ID was used

const uint8\_t invalidFontId = 0x05; // bkcmd 2,3 0x05 0xFF 0xFF 0xFF Returned when invalid Font ID was used

const uint8\_t invalidFileOperation = 0x06; // bkcmd 2,3 0x06 0xFF 0xFF 0xFF Returned when File operation fails

const uint8\_t invalidCrc = 0x09; // bkcmd 2,3 0x09 0xFF 0xFF 0xFF Returned when Instructions with CRC validation fails

// their CRC check

const uint8\_t invalidBaudRateSetting = 0x11; // bkcmd 2,3 0x11 0xFF 0xFF 0xFF Returned when invalid Baud rate was used

const uint8\_t invalidWaveformIdChan = 0x12; // bkcmd 2,3 0x12 0xFF 0xFF 0xFF Returned when invalid Waveform ID or Channel # was used

const uint8\_t invalidVarNameAttrib = 0x1A; // bkcmd 2,3 0x1A 0xFF 0xFF 0xFF Returned when invalid Variable name or invalid

// attribute was used

const uint8\_t invalidVarOperation = 0x1B; // bkcmd 2,3 0x1B 0xFF 0xFF 0xFF Returned when Operation of Variable is invalid.

// ie: Text assignment t0.txt = abc or t0.txt = 23,

// or Numeric assignment j0.val = ”50? or j0.val = abc

const uint8\_t assignmentFailed = 0x1C; // bkcmd 2,3 0x1C 0xFF 0xFF 0xFF Returned when attribute assignment failed to assign

const uint8\_t EEPROMOperationFailed = 0x1D; // bkcmd 2,3 0x1D 0xFF 0xFF 0xFF Returned when an EEPROM Operation has failed

const uint8\_t invalidQtyParams = 0x1E; // bkcmd 2,3 0x1E 0xFF 0xFF 0xFF Returned when the number of instruction parameters is

// invalid

const uint8\_t ioOperationFailed = 0x1F; // bkcmd 2,3 0x1F 0xFF 0xFF 0xFF Returned when an IO operation has failed

const uint8\_t invalidEscapeChar = 0x20; // bkcmd 2,3 0x20 0xFF 0xFF 0xFF Returned when an unsupported escape uint8\_tacter is used

const uint8\_t variableNameToLong = 0x23; // bkcmd 2,3 0x23 0xFF 0xFF 0xFF Returned when variable name is too long.Max length is

// 29 characters: 14 for page + “.” + 14 for component.

const uint8\_t serialBufferOverflow = 0x24; // always 0x24 0xFF 0xFF 0xFF Returned when a Serial Buffer overflow occurs

// Buffer will continue to receive the current instruction,

// all previous instructions are lost.

/\*

\* Error code generated by this library when incorrect number of characters returned by Nextion

\*/

const uint8\_t errorReadingNumber\_1 = 0x3D;

const uint8\_t errorReadingNumber\_2 = 0x3E;

const uint8\_t invalidNumCharsReturned = 0x3F;

enum bkcmdStateType {

noReturn,// = 0,

onSuccess, // = 1,

onFailure, // = 2 Default

always // = 3

};

const uint8\_t boilerButton = 5;

const uint8\_t hwButton = 6;

class Stream;

class Nextion {

public:

typedef void (\*setNextionBaudCallbackFunc) (uint32\_t); // create function pointer type

typedef void (\*nextionTurnValveOnOffCallbackFunc) (uint32\_t, bool); // create function pointer type

typedef void (\*setMcuDateTimeCallbackFunc) (); // create function pointer type

typedef void (\*systemResetCallbackFunc) (); // create function pointer type

const char revision[5] = "1.72";

const uint16\_t revisionNum = 172;

uint32\_t baudRate = 9600;

const uint32\_t resetNextionBaud = baudRate;

uint32\_t recoveryBaudRate = baudRate; // used for recovery when changing baud rate does not work

bool nextionError = false;

bool comdExecOk = false; // only used for bkcmd = 1 or 3

bool stringWaiting = false;

uint8\_t errorCode = instructionSuccess;

bkcmdStateType bkcmd = onFailure;

uint32\_t getNumVarTimeout = 1000;

uint32\_t getStrVarTimeout = 1000;

uint32\_t getEPromDataTimeout = 1000;

bool eepromDataChanged = true;

bool nextionDateTimeUpdt = false;

uint32\_t packedDateTime = 0;

int32\_t sndDateTimeHotSPage = 0;

bool daylightSaving = false;

nextionEventType nextionEvent;

Nextion(Stream\* s); // s is the serial stream to use e.g. Serial1

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* `` \*

\* Description of Nextion Public Variables \*

\* \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* \*

\* baudRate = 9600; The baud rate used for Nextion Comms. \*

\* resetNextionBaud = baudRate; The baud rate used after a reset. Needs to match \*

\* the value used in Program.s if changed from the default 9600\*

\* recoveryBaudRate = baudRate; Used for recovery when changing baud rate doesn't work. \*

\* nextionError = false; Returns true if a Nextion error has occured \*

\* comdExecOk = false; // only used for bkcmd = 1 or 3 \*

\* stringWaiting = false; Returns true if a string has been collected from Nextion. \*

\* errorCode = instructionSuccess; Error code returned if nextionError is true. \*

\* bkcmd = onFailure; NOT TESTED FOR CHANGE FROM THIS DEFAULT SETTING. \*

\* getNumVarTimeout = 1000; Timeout (mS) for getting numeric value from Nextion \*

\* getStrVarTimeout = 1000; Timeout (mS) for getting string result from Nextion \*

\* getEPromDataTimeout = 1000; Timeout (mS) for getting Eeprom data from Nextion. \*

\* eepromDataChanged = true; Returns true if Eeprom data has changed and should be read \*

\* from Nextion using getEEPromData. \*

\* Using this sets eepromDataChanged to false. \*

\* packedDateTime = 0; The variable used to hold the packed date/time returned \*

\* from the Nextion. \*

\* nextionDateTimeUpdt = false; The date/time has been changed on the Nextion. \*

\* and automatically collected into packedDateTime. \*

\* If setMcuDateTimeCallback() has been used the CallBack fn \*

\* will be used to set the mcuDate/Time. \*

\* If false getDateTime() will need to be used to get the \*

\* date/time. \*

\* This will set nextionDateTimeUpdt to false. \*

\* sndDateTimeHotSPage = 0 The page nuumber holding the sndDateTime Hotspot. \*

\* daylightSaving = false Set when time from Nextion packedDateTime decoded. \*

\* \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* \*

\* Description of Nextion functions \*

\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* begin(uint32\_t br, setNextionBaudCallbackFunc func = nullptr) - passes the Nextion \*

\* baud rate to the library. This is put into the variable baudRate. No changes to the \*

\* baudRate are made by this Function. Also, if passed, sets the call back function \*

\* so that this library can have control over the Teensy baudrate. \*

\* Turns on automatic control of Teensy baudrate if passed. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* begin( baudRate ) - autoSetting of Teensy baud rate set off. \*

\* begin( baudRate, setNextionBaud ) - passes the baud rate and function to change \*

\* Teensy baudRate. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void begin(uint32\_t br, setNextionBaudCallbackFunc func = nullptr);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* sendCommand(const char\* command); - Sends command to Nextion. \*

\* sendCommand(const char\* command, uint32\_t num); - Sends command & num to Nextion. \*

\* sendCommand(const char\* command, uint32\_t txt, encloseText); - Sends command & txt \*

\*--------------------------------------------------------------------------------------------------------\*

\* In the 3rd form above, if encloseTxt is true then txt is enclosed between \*

\* quotation marks ". \*

\* So sendCommand( "page0.CommentBox.txt=","Hello There",true); results in \*

\* page0.CommentBox.txt="Hello There"\xFF\xFF\xFF being sent to the Nextion. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Sends the command to Nextion. If bkcmd level has been set to 1 or 3 the code is \*

\* setup to look for a response from the Nextion. \*

\* if bkcmd set to 1 or 3, use the command lastComdCompletedOk(uint32\_t timeout) \*

\* below after a command or before the next command to determine that the (last) \*

\* command completed ok. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void sendCommand(const char\* command);

void sendCommand(const char\* command, uint32\_t num);

void sendCommand(const char\* command, const char\* txt, bool encloseText);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setBkCmdLevel(bkcmdStateType level) - Sets Nextion bkcmd value \*

\*--------------------------------------------------------------------------------------------------------\*

\* The default value is onFailure (2) \*

\* When set to 1 or 3, use the command bool lastComdCompletedOk(uint32\_t timeout) \*

\* below after a command or before the next command to determine that the (last) \*

\* command completed ok. \*

\* level is ONLY allowed to be 1 or 3 if compiled with #define bkcmd1or3allowed in \*

\* Nextiopn.cpp. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setBkCmdLevel(bkcmdStateType level);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setNextionBaudRate(uint32\_t br) - Sets the baud rate on Nextion and Teensy. \*

\*--------------------------------------------------------------------------------------------------------\*

\* This routine saves the current baud rate in a variable recoveryBaudRate so that \*

\* this recoveryBaudRate can be tried first by the recoverNextionComms() function \*

\* thus saving some time in the recovery. \*

\* In order for this function to work correctly it requires that the \*

\* setNextionBaudCallbackFunc was passed to the Library with the Nextion.display.begin \*

\* function. If not it will be the responsibility of the calling program to set the \*

\* Teensy BaudRate accordingly. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setNextionBaudRate(uint32\_t br);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* lastComdCompletedOk(uint32\_t timeout) - ret true/false if last comd completed ok \*

\*--------------------------------------------------------------------------------------------------------\*

\* This command is to be used if bkcmd level is set to 1 or 3 and ONLY where a \*

\* command is used to set a state on the Nextion. \*

\* Where a request for information is sent to nextion, as in "get varName", the \*

\* returned value is the handshake. \*

\* If other values are used (0 or 2) it is transparent and will return true. \*

\* This is not an indication that the command completed ok as handshaking is off. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool lastComdCompletedOk(uint32\_t timeout);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* Set the Text Area to be used for the Return of Text data from Nextion \*

\* If text is sent from the Nextion (following the 0x70 identifier) it will be \*

\* sent to SerialUsb if this function has not been used to specify a variable \*

\* to hold the text data. The parameter must be the size of the textBuffer \*

\* variable. If more text is returned than there is space for in textBuffer \*

\* it will be sent to the SerialUsb. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: setTextBuffer( textBuffer, sizeof( textBuffer )); \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setTextBuffer(/\*const\*/ char\* textBuffer, uint8\_t textBufferSize);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* Set the EEProm Data Area to be used for the Return of EEProm data from Nextion by \*

\* the fn bool getEEPromData(uint32\_t start, uint32\_t len) \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: setEEPromDataBuffer( eepromDataBuffer, sizeof(eepromDataBuffer)); \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setEEPromDataBuffer(/\*const\*/ char\* eepromDataBuffer, uint8\_t eepromBufferSize);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* clearBuffer() - Clears the Teensy (Nextion) serial input. \*

\* Use where things have perhaps gone wrong and you need to clear out erroneous \*

\* replies. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void clearBuffer();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* commsOk() - Checks that valid communications exist with the Nextion Display. \*

\* It sends the command "sendme\xFF\xFF\xFF" and looks for a reply. It does not look \*

\* for the page number for a reply, because comms may have been lost due to using \*

\* the wrong baud rate, in which case a reply might be 0x23FFFFFF - variable name \*

\* too long or some other error reply. Instead it looks for any valid reply. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool commsOk();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* reset(baudRate) - Resets the Nextion Display and sets the baud rate to "baudRate" \*

\*--------------------------------------------------------------------------------------------------------\*

\* Sends a reset command to the Nextion. Sets the Teensy baud rate to 9600 if that \*

\* baud rate NOT already in use. ( upon reset the Nextion defaults to this baud rate ) \*

\* and waits for a valid reply. The Teensy baud rate is set using the callBack \*

\* function registered using the display.begin function. \*

\* When a valid reply has been seen the Nextion AND Teensy have the buadRate changed \*

\* to the baud rate passed in the function call. \*

\* The function returns true if valid comms with the Nextion can be established. \*

\* Sets bkcmd to onFailure (Default) \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* reset() - If no baud rate is passed then the baudRate defaults to the reset 9600 \*

\* reset(1) - Sets the Baud Rate to that in use at the entry to the Reset function. \*

\* reset(115200) - Will do a reset and set the baudRate to 115200. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool reset(uint32\_t br = 0);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* recoverNextionComms() - attempts to recover Nextion Comms once they have been lost \*

\*--------------------------------------------------------------------------------------------------------\*

\* First sets the Teensy baud rate to the recoverBaudRate (see setNextionBaudRate \*

\* below). Uses the commsOK function to determine that comms have been re-established. \*

\* If that does not work then all the baud rates that the Nextion might use are cycled \*

\* through until a valid baud rate can be found. \*

\* Returns the value of the baud rate found. \*

\* If NO valid baud rate can be found then returns 0. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

uint32\_t recoverNextionComms();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* Check if char(s) returned from Nextion. If not do something else and come back \*

\* later to check again. Wait for timeout. Default is 0..don't wait. \*

\*--------------------------------------------------------------------------------------------------------\*

\* If there is a reply from Nextion then the Reply Char is received and the required \*

\* number of following char/bytes dependent upon the value of the Id. \*

\* The Id char is placed in nextionEvent.id. \*

\* The remaining chars are placed in nextionEvent.reply8 ready to be decoded. \*

\* True is returned if there is an Id char and the required number of chars \*

\* are returned. Otherwise, false is returned. \*

\* If the first char is received within timeout a further timeout of 1 second \*

\* is allowed for remaining characters. \*

\* This proc does NOT get any strings returned from Nextion,Use respondToReply() \*

\* for that. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool getReply(uint32\_t timeout = 0);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* respondToReply() - returns true if something needs responding to. \*

\*-------------------------------------------------------------------------------------------\*

\* This is where you need to put your code. Use getReply() to get any info from the \*

\* Nextion (see above) and this function to decode the reply and respond to it. \*

\* It returns true if further response is needed. \*

\*--------------------------------------------------------------------------------------------------------\*

\* I like to have requests from the Nextion Display embedded into numbers. Within this \*

\* code I want to turn valves on or off. The number returned by the Nextion contains \*

\* the valve to be moved and whether it should be opened or closed (0 or 1) \*

\* If you have handled the Nextion response fully then set needsResponse to false. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool respondToReply();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* printAnyReturnCharacters(uint32\_t nextionTime, uint8\_t id). \*

\* This function is intended to be used in debugging your code. It prints out to the \*

\* SerialUsb the value "nextionTime" and "Id", both values that might be useful in \*

\* tracking down where your error occurred, followed by any values that are in the \*

\* Serial input stream from the Nextion. \*

\* It might be that you have used "respondToReply", with your code in it, but still \*

\* there is something being returned that needs to be responded to. Use this function \*

\* to see what unexpected data is being sent from the Nextion Display. \*

\* ALL data is output in HEX. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void printAnyReturnCharacters(uint32\_t nextionTime, uint8\_t id);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setNextionBaudRate(uint32\_t br) - Sets the baud rate on Nextion and Teensy. \*

\*--------------------------------------------------------------------------------------------------------\*

\* This routine saves the current baud rate in a variable recoveryBaudRate so that \*

\* recoveryBaudRate can be tried first by the recoverNextionComms() function, \*

\* thus saving some time in the recovery. \*

\* In order for this function to work correctly it requires that the \*

\* setNextionBaudCallbackFunc was passed to the Library with the Nextion.display.begin \*

\* function. If not it will be the responsibility of the calling program to set the \*

\* Teensy BaudRate accordingly. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setNextionBaudRate(uint32\_t br);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* gotoPage(uint32\_t which); - Sets which is active displayed page. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void gotoPage(uint32\_t which);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* getPage(); - Returns the number of the active displayed page. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

int32\_t getPage();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setBackLight(uint32\_t backLight) - Sets the display BackLight(0..100). \*

\*--------------------------------------------------------------------------------------------------------\*

\* Any value greater than 100 will default to 100. \*

\* 0 is off 100 is MAX brightness. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setBackLight(uint32\_t backLight);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* getNumVarValue(const char\* varName) - Gets the value of Nextion Variable. \*

\* getNumVarValue(const char\* varName, const char\* suffixName) - Gets the value \*

\* of the Variable suffix. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Waits for up to 1000ms for a reply. If no reply returns -1. \*

\* The wait time is controlled by the variable getNumVarTimeout which is \*

\* initially set to 1000 ms. \*

\* Since -1 can alse be a valid return value nextionError is set on error and \*

\* the error is reported in errorCode as errorReadingNumber\_1 or \*

\* errorReadingNumber\_2 dependant upon which form of getNumVarValue is used. \*

\*--------------------------------------------------------------------------------------------------------\*

\* In reality this command should only be sent when the Nextion Serial buffer is \*

\* empty, otherwise, any reply may be from previously stacked up Nextion commands \*

\* and therefore be erroneous. \*

\*--------------------------------------------------------------------------------------------------------\*

\* In the second case returns the value of a variable suffix as in: \*

\* getNumVarValue( "x0","ws1") to get the number of dp for a Nextion float variable. \*

\* NOTE that the "." in "x0.ws1" is provided by the function. \*

\*--------------------------------------------------------------------------------------------------------\*

\* NOTE that, if appropriate, the ".val" varName suffix MUST be sent. Program.S \*

\* variables DO NOT need the ".val" suffix whereas Nextion Display variables do. \*

\* \*

\* For example to get a sys value just use getNumVarValue("sys"); but for a Display \*

\* variable va2, use getNumVarValue("va2.val"); OR getNumVarValue("va2","val"); \*

\*--------------------------------------------------------------------------------------------------------\*

\* The varName MUST exist. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

int32\_t getNumVarValue(const char\* varName);

int32\_t getNumVarValue(const char\* varName, const char\* suffixName);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* getNumVarFloat(const char\* varName) - Gets the value of Nextion Float Variable. \*

\*--------------------------------------------------------------------------------------------------------\*

\* getNumVarFloat uses getNumVarValue to get the various components of a Nextion \*

\* float. Wait times will be a combination of the two betNumVarValue wait times. \*

\* If an error occurs nextionError will be set to true and the returned value \*

\* should NOT be relied upon. \*

\* The error is reported in errorCode as errorReadingNumber\_2 \*

\*--------------------------------------------------------------------------------------------------------\*

\* In reality this command should only be sent when the Nextion Serial buffer is \*

\* empty otherwise, any reply may be from previously stacked up Nextion commands \*

\* and therefore be erroneous. \*

\* The varName MUST exist. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

float\_t getNumVarFloat(const char\* varName);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* getStringVarValue(const char\* varName) - Gets the text from Nextion Variable. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Waits for up to 1000ms for a reply. If no reply returns false. \*

\* The wait time is controlled by the variable getStrVarTimeout which is initially \*

\* set to 1000 ms. \*

\*-------------------------------------------------------------------------------------------\*

\* In reality this command should only be sent when the Nextion Serial buffer is \*

\* empty, otherwise any reply may be from previously stacked up Nextion commands \*

\* and therefore be erroneous. \*

\* The varName MUST exist. \*

\*--------------------------------------------------------------------------------------------------------\*

\* The result is placed in the string setup with the setTextBuffer function. \*

\* If no string has been setup it will simply be echoed to the screen (Serial). \*

\* Returns true if string returned successfully. stringWaiting is also set to true. \*

\*--------------------------------------------------------------------------------------------------------\*

\* NOTE there is no need to send the ".txt" suffix to the string variable. \*

\* getStringVarValue("va0") will send "get va0.txtFFFFFF" to the Nextion and wait for \*

\* an answer. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool getStringVarValue(const char\* varName);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* bool getEEPromData(uint32\_t start, uint32\_t len) - Gets the EEProm data from start for \*

\* len bytes.\*

\*--------------------------------------------------------------------------------------------------------\*

\* Waits for up to 1000ms for a reply. If no reply returns false. \*

\* The wait time is controlled by the variable getEPromDataTimeout which is initially set to \*

\* 1000 ms. \*

\*--------------------------------------------------------------------------------------------------------\*

\* In reality this command should only be sent when the Nextion Serial buffer is \*

\* empty, otherwise any reply may be from previously stacked up Nextion commands \*

\* and therefore be erroneous. \*

\*------------------------------------------------------------------------------------------- \*

\* The result is placed in the EEPromDataBuffer setup with the setEEPromDataBuffer \*

\* fn returned true if len bytes collected. The number of bytes collected is placed in \*

\* the global variable eepromBytesRead. \*

\* A valid getEpromData also sets eepromDataChanged to false. \*

\* Initially it is set to true to force initial collection of Nextion eeprom data. \*

\* If no EEPromDataBuffer has been setup it will simply return false. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool getEEPromData(uint32\_t start, uint8\_t len);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setNumVarValue(const char\* varName, int32\_t var ) - Sets Nextion Variable to var. \*

\*--------------------------------------------------------------------------------------------------------\*

\* NOTE that, if appropriate, the ".val" varName suffix MUST be sent. Program.S \*

\* variables DO NOT need the ".val" suffix whereas Nextion Display variables do. \*

\*--------------------------------------------------------------------------------------------------------\*

\* For example to set a sys value just use setNumVarValue("sys",100); but for a \*

\* display variable va2, use setNumVarValue("va2.val",100); \*

\*--------------------------------------------------------------------------------------------------------\*

\* The varName MUST exist. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool setNumVarValue(const char\* varName, int32\_t var);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* bool setNumVarFloat(const char\* varName, float\_t fvar, uint8\_t dp, bool round) \*

\* - Sets Nextion Variable to fvar, with dp decimal points rounded to dp (or not). \*

\*--------------------------------------------------------------------------------------------------------\*

\* NOTE that the ".val" varName suffix MUST NOT be sent. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* if (display.setNumVarFloat( "x0", 1234.5678, 2, true ) {.... displays 1234.57 in x0.\*

\* if (display.setNumVarFloat( "x0", 1234.5678, 2, false ) {... displays 1234.56 in x0.\*

\*--------------------------------------------------------------------------------------------------------\*

\* The varName MUST exist. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool setNumVarFloat(const char\* varName, float\_t fvar, uint8\_t dp, bool round);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setStrVarValue(const char\* varName, const char\* var ) - Sets String Variable to var. \*

\*--------------------------------------------------------------------------------------------------------\*

\* NOTE that there is no need to send the variable suffix ".txt". \*

\* setStrVarValue("va0","this is a string") will send: \*

\* va0.txt="this is a string"FFFFFF to the Nextion. \*

\*--------------------------------------------------------------------------------------------------------\*

\* The varName MUST exist. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool setStrVarValue(const char\* varName, const char\* var);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* askSerialBufferClear() - Ask Nextion if Serial Buffer Clear (Empty) \*

\*--------------------------------------------------------------------------------------------------------\*

\* Sends "get clrBufr" to Nextion. Nextion will reply with 0xFDFD when it gets to \*

\* this request in the SerialBuffer, indicating it has executed this last command \*

\* in the Serial Buffer. If other commands are sent after this one the Serial \*

\* Buffer WILL NOT BE CLEAR. \*

\* Use the command isSerialBufferClear(), below to confirm Serial Buffer Clear. \*

\* Requires this line "int clrBufr=65021" in Nextion Program.s \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void askSerialBufferClear();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* isSerialBufferClear() - Query answer from askSerialBufferClear() above \*

\*--------------------------------------------------------------------------------------------------------\*

\* NOTE that if other commands are stacked up which will give a reply from Nextion, \*

\* then they will be handled by the calls to getReply and respondToReply used by \*

\* this function. They may return a reply, but if it is NOT a Numeric reply with \*

\* 0xFDFD they will NOT return true. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool isSerialBufferClear();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* bool askSerialBufferClear(uint32\_t timeout) - As above but waits for a reply \*

\*--------------------------------------------------------------------------------------------------------\*

\* Combines askSerialBufferClear() and isSerialBufferClear() with a timeout to \*

\* determine if the Nextion input Serial Buffer is Clear. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool askSerialBufferClear(uint32\_t timeout);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* turnNextionButton(uint8\_t which, bool on) \*

\* I have Nextion buttons named Sw0..Sw6. I use this function to set the relevant \*

\* button on (1) or off (0) \*

\* I have ghosted this function with the phrase "turnNextionValve" since some of the \*

\* buttons are controlling valves and it makes more sense in the code to refer to \*

\* them as valves. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

#define turnNextionValve turnNextionButton

void turnNextionButton(uint8\_t which, bool on);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setHotWaterOnForMins(uint8\_t howLong) \*

\*--------------------------------------------------------------------------------------------------------\*

\* This is somewhat clever. Teensy sets the hot water on and sends a command to the \*

\* Nextion to turn off the hot water in "howLong" minutes. \*

\* When the Nextion receives this command (via a numeric value in a Number Variable) \*

\* it turns the display for the valve open "on" and when the timeout occurs it sends \*

\* a command to the Teensy to turn off the hot water. This is done via the callback \*

\* setup via the setValveCallBack(nextionTurnValveOnOffCallbackFunc func)function. \*

\* Thus some timing control is offloaded to the Nextion. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setHotWaterOnForMins(uint8\_t howLong);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setTime(uint32\_t time) - Sets the time on the Nextion. \*

\*--------------------------------------------------------------------------------------------------------\*

\* The time is sent as HEX HHMMSS in the variable "SetTime=HHMMSS0xFF0xFF0xFF" \*

\* When the Nextion sees that SetTime is not zero it sets the Nextion time. \*

\* The SetTime variable is then set to 0. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* uint32\_t time = Hours \* 0x10000 + Minutes \* 0x100 + Seconds \*

\* display.setTime(time) \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setTime(uint32\_t time);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setDate(uint32\_t date) - Sets the date on the Nextion. \*

\*--------------------------------------------------------------------------------------------------------\*

\* The time is sent as HEX YYMMDD in the variable "page0.SetDate=YYMMDD0xFF0xFF0xFF" \*

\* When the Nextion sees that StDate is not zero it sets the Nextion date. \*

\* The StDate variable is then set to 0. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* uint32\_t date = (Year-2000) \* 0x10000 + Month \* 0x100 + Day \*

\* display.setDate(date) \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setDate(uint32\_t date);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* getDateTime() - Gets the date and Time from Nextion. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Gets the Date/Time set in the Nextion. \*

\* The packed date/time is placed in the global variable packedDateTime. \*

\* It can be decoded as shown below: \*

\*--------------------------------------------------------------------------------------------------------\*

\* dow = packedDateTime >> 29; // (sun=0) \*

\* dst = ( packedDateTime >> 28 ) & 0x01; (known as BST in the UK) \*

\* year = ( packedDateTime >> 21 ) & 0x7F + 2000; \*

\* month = ( packedDateTime >> 17 ) & 0x0F; \*

\* day = ( packedDateTime >> 12 ) & 0x1F; \*

\* hour = ( packedDateTime >> 6 ) & 0x1F; \*

\* minute = ( packedDateTime ) & 0x3F; \*

\*--------------------------------------------------------------------------------------------------------\*

\* NOTE: This fn should only be called when the page holding the hotspot SndDateTime \*

\* is displayed. On the new example HMI file it is on page 0. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* display.getDateTime() \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool getDateTime();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* turnDebugOn(bool on) - Turn Nextion debug variable on or off \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* turnDebugOn( true ) - Turn debug on \*

\* turnDebugOn( false ) - Turn debug off \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool turnDebugOn(bool on);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setScreenDimTime(uint32\_t dimTime) - Sets the time, in seconds, after which the \*

\* screen will dim if screen dimming is turned on. \*

\* The default is 3 minutes. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool setScreenDimTime(uint32\_t dimTime);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* turnScreenDimOn(bool on) - Turn Nextion dimAllowed variable on or off \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* turnScreenDimOn( true ) - Turn Dim on \*

\* turnScreenDimOn( false ) - Turn Dim off \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool turnScreenDimOn(bool on);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* printAnyReturnCharacters(uint32\_t nextionTime, uint8\_t id). \*

\* This function is intended to be used in debugging your code. It prints out to the \*

\* SerialUsb the value "nextionTime" and "Id", both values that might be useful in \*

\* tracking down where your error occurred, followed by any values that are in the \*

\* Serial input stream from the Nextion. \*

\* It might be that you have used "respondToReply", with your code in it, but still \*

\* there is something being returned that needs to be responded to. Use this function \*

\* to see what unexpected data is being sent from the Nextion Display. \*

\* ALL data is output in HEX. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void printAnyReturnCharacters(uint32\_t nextionTime, uint8\_t id);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setValveCallBack(nextionTurnValveOnOffCallbackFunc func) - passes the Nextion the \*

\* call back function tu turn a valve on or off \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setValveCallBack(nextionTurnValveOnOffCallbackFunc func);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setMcuDateTimeCallback(setMcuDateTimeCallbackFunc func) - passes the Nextion the \*

\* call back fn to Set the MCU date and time. It also sets autoUpdateDateTime to true. \*

\* This setMcuDateTimeCallbackFunc is called when Nextion reports a change in date/time \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setMcuDateTimeCallback(setMcuDateTimeCallbackFunc func);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setSystemResetCallback(systemResetCallbackFunc func) - passes the Nextion the \*

\* call back fn to carry out a System Reset. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setSystemResetCallback(systemResetCallbackFunc func);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setLedState - Sets the state of the leds in top, middle or bottom Row. \*

\* which = led (0..7) and state is on (1), off (0) or flashing (2). \*

\*--------------------------------------------------------------------------------------------------------\*

\* Just sets the state in variable holding leds row state. There is no change \*

\* to the leds display until setNextionLeds( row ) is used. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: setLedState( mid, 4, flashing ); \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setLedState(topMidBottmType whichLed, uint8\_t which/\*0..7\*/, onOffFlashingType state);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setNextionLeds actually sends command to Nextion to change the state of \*

\* which leds ( top, middle or bottom row ) set with setLedState function above. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: setNextionLeds( top ); \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void setNextionLeds(topMidBottmType which);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* clearLeds sets the leds state variable to all (top, middle and bottom) off. \*

\* Uses setNextionLeds to send command to update all rows on Nextion. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void clearLeds();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* printTimeEmbeddedTextToNextion - Sends Text to Nextion to be placed in variable \*

\* page0.msg.txt. If transmit is set to true the text is terminated with a " \*

\* character and m0,1 is clicked to cause the screen on page1 to be updated using \*

\* the finishNextionTextTransmittion() command (see below). \*

\* The procedure sends page0.msg.txt=" to the Nextion followed by the text. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: printTimeEmbeddedTextToNextion( "This is a load of text for page1", true ); \*

\*--------------------------------------------------------------------------------------------------------\*

\* A string representing the Nextion time in the format " HH:MM:SS " is inserted \*

\* AFTER the first character. This is carried out by the Nextion display. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void printTimeEmbeddedTextToNextion(const char\* p, bool transmit);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* printTextToNextion - Sends Text to Nextion to be placed in variable \*

\* page1.va0.txt. If transmit is set to true the text is terminated with a " \*

\* character and m0,0 is clicked to cause the screen on page1 to be updated using \*

\* the finishNextionTextTransmittion() command (see below). \*

\* The procedure sends page1.va0.txt=" to the Nextion followed by the text. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: printTextToNextion( "This is a load of text for page1", true ); \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void printTextToNextion(const char\* p, bool transmit);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* printMoreTextToNextion - It is the same as the printTextToNextion function except \*

\* that the page0.msg.txt=" is NOT sent. \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: printMoreTextToNextion( "This is a load of text for page1", true ); \*

\* NOTE: DO NOT use this without first using printTextToNextion( "text", false ); \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void printMoreTextToNextion(const char\* p, bool transmit) {

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* printNumericText - Sends number to Nextion. This command MUST have been preceded \*

\* by the printTextToNextion command shown above. If transmit is set to true the text \*

\* is terminated with a "character and m0 is clicked to cause the screen on page1 to \*

\* be updated using the finishNextionTextTransmittion() command (see below). \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: printNumericText( n, true ); // where n is a uint32\_t \*

\* NOTE: DO NOT use this without first using printTextToNextion( "text", false ); \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void printNumericText(uint32\_t num, bool transmit);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* finishNextionTextTransmittion() - Terminate the text transmitted to Nextion with a \*

\* " character and terminate the command correctly. Also issues the relevant \*

\* click m0 command dependant upon which printText command was used to cause the \*

\* screen on page1 to be updated. \*

\* ( Uses "click m0,1" or "click m0,0" as appropriate ) \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: finishNextionTextTransmittion() \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void finishNextionTextTransmittion();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* I like to keep a monitor of what has happened in the system. This display is on \*

\* page1 of the Nextion display. I use the first character position to indicate the \*

\* type of message/source of message. e.g. C for command, E for error message. After \*

\* this character I inser the Time in " HH:MM:SS " format. This is done by the \*

\* Nextion Display. \*

\*--------------------------------------------------------------------------------------------------------\*

\* printCommandOrErrorTextMessage - sends the commandOrError charater followed by the \*

\* textMessage to the Nextion using the printTextToNextion command above. \*

\* If transmit is set to true the text is terminated with a "character and m0 is \*

\* clicked to cause the screen on page1 to be updated using the \*

\* finishNextionTextTransmittion() command (see above). \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void printCommandOrErrorTextMessage(const char\* commandOrError, const char\* textMessage, bool transmit);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* preserveTopTextLine() - Top text line writing inhibited. \*

\*--------------------------------------------------------------------------------------------------------\*

\* All general text commands do not use top line if this command actuated. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void preserveTopTextLine();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* writeToTopTextLine(const char\* textMessage) \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void writeToTopTextLine(const char\* textMessage);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* releaseTopTextLine() - Allows writing to the Top Text Line \*

\*--------------------------------------------------------------------------------------------------------\*

\* All general text commands can use top line again (Default Setting). \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void releaseTopTextLine();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* clearTextScreen()- Clears the Nextion Text Screen (page1) \*

\*-------------------------------- ------------------------------------------------------------------------\*

\* If the Top Line is preserved that is not cleared, use clearTopTextLine instead. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void clearTextScreen();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* clearTopTextLine() - Clears the Nextion Text Screen Top Text Line \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void clearTopTextLine();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* setDaylightSavingOn( on) - Turn Nextion daylight saving variable on or off \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* setDaylightSavingOn( true ) - Turn on \*

\* setDaylightSavingOn( false ) - Turn off \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool setDaylightSavingOn( bool on);

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* getDaylightSavingOn() - Returns Nextion daylight saving variable (true=on) \*

\*--------------------------------------------------------------------------------------------------------\*

\* Usage: \*

\* getDaylightSavingOn() \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

bool getDaylightSavingOn();

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* viewDebugText(bool view) - Displays the debugTxt Text Line (or NOT) \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

void viewDebugText(bool view);